Leakage curretn at 350V normalized to 20degC0501001502002503003504000100200300400500600Leakage current (nA)

Number of sensors