1) 12-Chip Full Electrical Module- 4 n-on-n ATLAS97 novel p-stopdetectors, matching the n-ABCDchips.- Double-side instrumented...12 chip hybrid with ’’ tested ’’ n-ABCD chip: the top 6 chips were’’ Q-factor ’’ about 2 and the bottom6 chips ’’ Q-factor ’’ < 1 (no backsidemetallization) - First 4 channels were un-bonded out ofgroup of 32 channels.16 un-bonded/chip108 wire-bonded/chip (5th channel was excluded)- The Si detectors were biased at 200 V