2) Data Acquisition Setup-The setup used was the UCI DSP based hardwares:: Melbourne S C 9 7 for interfacing the hybrid and cable to the backend electronics: Cambridge BC96for supplying powers to the hybrid, merging the data cable fromSLL and the bias power supply to the detector: UCI SLL (Strip Low Level) cardfor the communication between the SC97 and the DSP: UCI VME-DSP modulefor the data processing and communication with V M E : 266 MHz Pentinum II PC with Windows NT4.0 OS.- PC-DAQ (abcdaq) software for the data acquisition: Data taking with Loop=1