Gain and Offset ( 4 ) - 1

>>SummaryofGain

F Ecurrent(mA) chipnumber errorbars rmsspreads